Imaxen:Dampflok-p8.jpg - Uiquipedia

# Imaxen:Dampflok-p8.jpg

### De Uiquipedia

- Imaxen
- Historia del archivu
- Enllaces a esta semeya
- Metadata

Size of this preview: 800 × 600 pixel
Image in higher resolution (1000 × 750 pixel, file size: 175 KB, MIME type: image/jpeg)

| Ésti ye un ficheru de Wikimedia Commons, un depósitu de conteníu llibre que tien la Fundación Wikimedia. Por favor consulte la so páxina de descripción allí pa ver la información sobre'l so orixen y llicencia.

en: Locomotive Prussian series P8 (German series 38); belonging to the railway museum Bochum-Dahlhausen

de: Dampflok - preußische P8; gehört zum Eisenbahnmuseum Bochum-Dahlhausen

Fotografiert von Bernd Untiedt - Januar 2002 / Author: Bernd Untiedt

(taken from the German Wikipedia [1]]

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Asturianu | Български | বাংলা | ইমার ঠার | Brezhoneg | Bosanski | Català | Sinugboanong Binisaya | Česky | Dansk | Deutsch | Ελληνικά | English | Esperanto | Español | Eesti | Euskara | فارسی | Suomi | Français | Galego | עברית | Hrvatski | Magyar | Bahasa Indonesia | Ido | Íslenska | Italiano | 日本語 | ქართული | 한국어 | Kurdî / كوردي | Latina | Lëtzebuergesch | Lietuvių | Bahasa Melayu | Nnapulitano | Nederlands | Norsk (nynorsk) | Norsk (bokmål) | Polski | Português | Română | Русский | Slovenčina | Slovenščina | Shqip | Српски | Svenska | తెలుగు | ไทย | Türkçe | Українська | اردو | Tiếng Việt | Volapük | 中文(简体) | 中文(繁體) | +/-

Dampflok-p8.jpg:Image:Dampflok-p8.jpg

{

## Enllaces a esta semeya

Les páxines siguientes enllacien a esti archivu:

- Ferrocarril

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | Canon
Camera model | Canon PowerShot G2
Orientation | Normal
Horizontal resolution | 180 dpi
Vertical resolution | 180 dpi
File change date and time | 11:24, 23 febreru 2002
Y and C positioning | 1
Exposure time | 1/50 sec (0.02)
F Number | f/2.5
Exif version | 2.1
Date and time of data generation | 11:24, 23 febreru 2002
Date and time of digitizing | 11:24, 23 febreru 2002
Mou de compresión d'imaxe | 5
Shutter speed | 5.65625
Aperture | 2.65625
Exposure bias | 0
Maximum land aperture | 2
Subject distance | 9.321 metres
Metering mode | Pattern
Flash | 0
Lens focal length | 10.6875 mm
Color space | sRGB
Focal plane X resolution | 8114.2857142857
Focal plane Y resolution | 8114.2857142857
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor

Retrieved from "http://ast.wikipedia.org../../../d/a/m/Imaxen%7EDampflok-p8.jpg_95f4.html"

##### Views

- semeya
- Discusión
- Revisión actual

##### Buscar