Imaxen:Puente Ingeniero Carlos Fernández Casado.jpg - Uiquipedia

# Imaxen:Puente Ingeniero Carlos Fernández Casado.jpg

### De Uiquipedia

- Imaxen
- Historia del archivu
- Enllaces a esta semeya
- Metadata

Size of this preview: 800 × 600 pixel
Image in higher resolution (2048 × 1536 pixel, file size: 725 KB, MIME type: image/jpeg)

| Ésti ye un ficheru de Wikimedia Commons, un depósitu de conteníu llibre que tien la Fundación Wikimedia. Por favor consulte la so páxina de descripción allí pa ver la información sobre'l so orixen y llicencia.

## [edit] Summary

Foto conseguida de http://www.asturlinux.org/galeria/berrueta-blog/IMG_3970 su autor es: http://www.asturlinux.org/~berrueta/ Comparto la foto en esta licencia porque el autor así me lo ha permitido (y pedido) con un correo electrónico. Es el puente Ingeniero Carlos Fernández Casado que cruza el embalse de Barrios de Luna, en la AP-66 (antes A-66), que es la autopista que va de León a Asturias, es un puente atirantado muy bonito.

## [edit] Licensing

| This file is licensed under the Creative Commons Attribution ShareAlike 2.5 License. In short: you are free to share and make derivative works of the file under the conditions that you appropriately attribute it, and that you distribute it only under a license identical to this one. Official license

## Enllaces a esta semeya

Les páxines siguientes enllacien a esti archivu:

- Autovía Ruta de la Plata

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | Canon
Camera model | Canon PowerShot A70
Orientation | Normal
Horizontal resolution | 180 dpi
Vertical resolution | 180 dpi
File change date and time | 10:06, 4 xunu 2005
Y and C positioning | 1
Exposure time | 1/400 sec (0.0025)
F Number | f/5.6
Exif version | 2.2
Date and time of data generation | 10:06, 4 xunu 2005
Date and time of digitizing | 10:06, 4 xunu 2005
Mou de compresión d'imaxe | 3
Shutter speed | 8.65625
Aperture | 4.96875
Exposure bias | 0
Maximum land aperture | 2.96875
Metering mode | Pattern
Flash | 16
Lens focal length | 5.40625 mm
Color space | sRGB
Focal plane X resolution | 9846.1538461538
Focal plane Y resolution | 9846.1538461538
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Scene capture type | Landscape

Retrieved from "http://ast.wikipedia.org../../../p/u/e/Imaxen%7EPuente_Ingeniero_Carlos_Fern%C3%A1ndez_Casado.jpg_19eb.html"

##### Views

- semeya
- Discusión
- Revisión actual

##### Buscar