# Berkas:Cartesian coordinates 2D.svg

### Dari Wikipedia Indonesia, ensiklopedia bebas berbahasa Indonesia.

- Berkas
- Versi terdahulu
- Pranala

Tak tersedia resolusi yang lebih tinggi.

Cartesian_coordinates_2D.svg‎ (800 × 742 piksel, ukuran berkas: 57 KB, tipe MIME: image/svg+xml)

| Berkas ini berasal dari Wikimedia Commons. Berikut ini adalah deskripsi berkas dari halaman deskripsi di sana.

## [edit] Summary

Example for en:Cartesian coordinate system. Created by Gustavb using en:PSTricks.

## [edit] Licensing

I, the author of this work, hereby publish it under the following license:

| Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Asturianu | Български | বাংলা | ইমার ঠার | Brezhoneg | Bosanski | Català | Sinugboanong Binisaya | Česky | Dansk | Deutsch | Ελληνικά | English | Esperanto | Español | Eesti | Euskara | فارسی | Suomi | Français | Galego | עברית | Hrvatski | Magyar | Bahasa Indonesia | Ido | Íslenska | Italiano | 日本語 | ქართული | 한국어 | Kurdî / كوردي | Latina | Lëtzebuergesch | Lietuvių | Bahasa Melayu | Nnapulitano | Nederlands | Norsk (nynorsk) | Norsk (bokmål) | Polski | Português | Română | Русский | Slovenčina | Slovenščina | Shqip | Српски | Svenska | తెలుగు | ไทย | Türkçe | Українська | اردو | Tiếng Việt | Volapük | 中文(简体) | 中文(繁體) | +/-

## [edit] Source

### [edit] Cartesian_coordinates_2D.tex (PSTricks source)

    \input pst-eps\input pst-plot\input pst-node\TeXtoEPS

    \psset{linecolor=black,linewidth=1pt,arrowsize=8pt,unit=0.29cm}
    \pspicture*(-15.3,-15.3)(17.4,15.3)

    % Axes
    \psaxes[Dx=5,Dy=5]{<->}(0,0)(-14.5,-14.5)(14.5,14.5)
    \psset{linewidth=.4pt}
    \psaxes[Dx=1,Dy=1,labels=none,ticksize=1.5pt](0,0)(-13,-13)(13,13)
    \uput{10pt}[0](0,14){\psscalebox{1.25}{\it y-axis}}
    \uput{10pt}[70](14,0){\psscalebox{1.25}{\it x-axis}}

    % Origin
    \pnode(0,0){O}
    \uput{35pt}[310](0,0){\rnode{Ot}{\psscalebox{1.1}{
            \vbox{\halign{\hfil#\hfil\cr$(0,0)$\cr\it origin\cr}}}}}
    \nccurve[angleA=315,angleB=145,arrowsize=4pt,
            nodesepA=2pt,nodesepB=-3pt,linecolor=gray]{<-}{O}{Ot}

    % Point
    \psdots[dotstyle=*,dotscale=1.2](3,5)
    \psline[linestyle=dotted,linewidth=.8pt](3,0)(3,5)(0,5)
    \uput{2.5pt}[53](3,5){\psscalebox{1.1}{$P(3,5)$}}

    % Quadrants
    \uput{3cm}[45](0,0){\psscalebox{1.6}{\bf I}}
    \uput{3cm}[135](0,0){\psscalebox{1.6}{\bf II}}
    \uput{3cm}[225](0,0){\psscalebox{1.6}{\bf III}}
    \uput{3cm}[315](0,0){\psscalebox{1.6}{\bf IV}}

    \endpspicture
    \endTeXtoEPS
    \nopagenumbers
    \end

### [edit] Instructions

1. Create EPS

       $ tex Cartesian_coordinates_2D.tex && dvips -E Cartesian_coordinates_2D.dvi

2. Outline fonts

       $ eps2eps -dNOCACHE Cartesian_coordinates_2D.ps Cartesian_coordinates_2D2.eps

3. Fix bounding box

       $ ps2epsi Cartesian_coordinates_2D2.eps Cartesian_coordinates_2D.eps

4. Convert to Sketch

       $ pstoedit -f sk Cartesian_coordinates_2D.eps Cartesian_coordinates_2D.sk

5. Convert to SVG

       $ skconvert Cartesian_coordinates_2D.sk Cartesian_coordinates_2D.svg

6. Fix `Cartesian_coordinates_2D.svg` with Inkscape

## Pranala

Halaman-halaman berikut memiliki pranala ke berkas ini:

- Sistem koordinat Kartesius

Diperoleh dari "http://id.wikipedia.org../../../c/a/r/Berkas%7ECartesian_coordinates_2D.svg_d5d5.html"

##### Views

- Berkas
- Pembicaraan
- Revisi sekarang

##### Cari