# 그림:Blue Marlin transporting sea-based X-band radar.jpg

### 위키백과 ― 우리 모두의 백과사전.

- 그림
- 파일 역사
- 그림 링크
- 메타데이터

Size of this preview: 800 × 571 pixel
Image in higher resolution (2100 × 1500 pixel, file size: 1.41 MB, MIME type: image/jpeg)

이 자료는 위키미디어 공용에 있습니다. 이 자료에 대한 설명이 아래에 있습니다.

Blue Marlin carrying sea-based x-band radar

## [edit] Caption from source

The heavy lift vessel MV Blue Marlin with its deck cargo of the Sea-Based X-Band Radar enters Pearl Harbor, Hawaii, after completing a 15,000-mile journey from Corpus Christi, Texas, on January 9, 2006.

Originally uploaded by Dual Freq on en.wikipedia.

## [edit] Source

http://www.defenselink.mil/photos/Jan2006/060109-N-3019M-012.html http://www.defenselink.mil/photos/Jan2006/060109-N-3019M-012.jpg

## [edit] License

DoD photo by Petty Officer 2nd Class Ryan C. McGinley, U.S. Navy. (Released)

- MDA got it from the navy, so changed to PD-USN

| This image is a work of a sailor or employee of the U.S. Navy, taken or made during the course of the person's official duties. As a work of the U.S. federal government, the image is in the public domain. |

Info:Sea-based X-band Radar

## 그림 링크

다음 문서들이 이 그림을 사용하고 있습니다:

- X밴드 레이더
- 지상 기반 외기권 방어

## 메타데이터

이 파일은 카메라/스캐너 정보와 같은 부가적인 정보를 담고 있습니다. 파일을 변경한다면 몇몇 세부 사항은 변경된 그림에 적용되지 않을 수 있습니다.

Camera manufacturer | NIKON CORPORATION
Camera model | NIKON D70s
Orientation | Normal
Horizontal resolution | 300 dpi
Vertical resolution | 300 dpi
Software used | Adobe Photoshop CS Macintosh
File change date and time | 2006년 1월 10일 (화) 14:51
Y and C positioning | 2
Exposure time | 1/1000 sec (0.001)
F Number | f/5.6
Exposure Program | Aperture priority
Exif version | 2.21
Date and time of data generation | 2006년 1월 9일 (월) 16:53
Date and time of digitizing | 2006년 1월 9일 (월) 16:53
Image compression mode | 4
Exposure bias | 0
Maximum land aperture | 5
Metering mode | Pattern
Light source | Unknown
Flash | 0
Lens focal length | 100 mm
DateTime subseconds | 10
DateTimeOriginal subseconds | 10
DateTimeDigitized subseconds | 10
Color space | sRGB
Sensing method | One-chip color area sensor
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Focal length in 35 mm film | 150
Scene capture type | Standard
Contrast | Normal
Saturation | Normal
Sharpness | Normal
Subject distance range | Unknown

원본 주소 ‘http://ko.wikipedia.org../../../b/l/u/%EA%B7%B8%EB%A6%BC%7EBlue_Marlin_transporting_sea-based_X-band_radar.jpg_0d12.html’

##### Views

- 그림
- 토론
- 현재 버전

##### 찾기