Image:South Wimbledon tube station surface building.jpg - Wikipedia

# Image:South Wimbledon tube station surface building.jpg

### From Wikipedia

- Image
- Stòria dal archivi
- Ligámm
- Metadata

Size of this preview: 800 × 600 pixel
Image in higher resolution (1600 × 1200 pixel, file size: 903 KB, MIME type: image/jpeg)

This file is a shared upload and may be used by other projects.

The surface building at South Wimbledon tube station on the Northern Line. Of all the London Underground stations, only Morden, also on the Northern Line, is further south.

I, Chris McKenna (en:User:Thryduulf), the creator of this work, hereby publish it under all Creative Commons Attribution ShareAlike (cc-by-sa) licenses, specifically including all national variations.

This file is licensed under the Creative Commons Attribution ShareAlike license versions 2.5, 2.0, and 1.0

العربية | Česky | Dansk | Deutsch | English | Español | فارسی | Français | Italiano | 日本語 | Nederlands | Polski | Português | Русский | Svenska | Türkçe | 简体中文 | 正體中文 | +/-

Derivitave works may be licensed under any Creative Commons license containing both Attribution (by) and ShareAlike (sa) license elements.
Please see User:Thryduulf/Relicensing if you wish to use this image under a different license.

## Ligámm

The following pages link to this file:

- South Wimbledon tube station

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | Panasonic
Camera model | DMC-FZ20
Orientation | Normal
Horizontal resolution | 72 dpi
Vertical resolution | 72 dpi
Software used | Ver1.0
File change date and time | 12:41, 15 ginee 2006
Y and C positioning | 2
Exposure time | 1/320 sec (0.003125)
F Number | f/4
Exposure Program | Normal program
ISO speed rating | 80
Exif version | 2.2
Date and time of data generation | 12:41, 15 ginee 2006
Date and time of digitizing | 12:41, 15 ginee 2006
Image compression mode | 4
Exposure bias | 0
Maximum land aperture | 3
Metering mode | Pattern
Light source | Unknown
Flash | 16
Lens focal length | 6 mm
Color space | sRGB
Sensing method | One-chip color area sensor
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 0
Focal length in 35 mm film | 36
Scene capture type | Standard
Contrast | Normal
Saturation | Normal
Sharpness | Normal

Utegnüü da "http://lmo.wikipedia.org../../../s/o/u/Image%7ESouth_Wimbledon_tube_station_surface_building.jpg_be69.html"

##### Views

- File
- Discüssiun
- Current revision

##### navegá

- Pagina prinçipala
- Purtaal wikipedista
- Grott
- Purtaal temàtech
- Atüalitaa
- Pàgin da jütt
- Dunazziun

##### Truvá