Attēls:Pensford and Viaduct.jpg - Vikipēdija

# Attēls:Pensford and Viaduct.jpg

### Vikipēdijas raksts

- Attēls
- Attēla hronoloģija
- Attēlu saites
- Metadata

Size of this preview: 800 × 600 pixel
Image in higher resolution (2272 × 1704 pixel, file size: 1,59 MB, MIME type: image/jpeg)

Šis fails ir no Wikimedia Commons. Skat. attēla apraksta lapu.

## [edit] Summary

Description | Pensford with Pensford Viaduct in the foreground
Source | Self
Date | 6th June 2006
Author | Self
Permission | n/a

## [edit] Licensing

I, the author of this work, hereby publish it under the following licenses:

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Asturianu | Български | বাংলা | ইমার ঠার | Brezhoneg | Bosanski | Català | Sinugboanong Binisaya | Česky | Dansk | Deutsch | Ελληνικά | English | Esperanto | Español | Eesti | Euskara | فارسی | Suomi | Français | Galego | עברית | Hrvatski | Magyar | Bahasa Indonesia | Ido | Íslenska | Italiano | 日本語 | ქართული | 한국어 | Kurdî / كوردي | Latina | Lëtzebuergesch | Lietuvių | Bahasa Melayu | Nnapulitano | Nederlands | Norsk (nynorsk) | Norsk (bokmål) | Polski | Português | Română | Русский | Slovenčina | Slovenščina | Shqip | Српски | Svenska | తెలుగు | ไทย | Türkçe | Українська | اردو | Tiếng Việt | Volapük | 中文(简体) | 中文(繁體) | +/-

This file is licensed under the Creative Commons Attribution ShareAlike license versions 2.5, 2.0, and 1.0

العربية | Česky | Dansk | Deutsch | English | Español | فارسی | Français | Italiano | 日本語 | Nederlands | Polski | Português | Русский | Svenska | Türkçe | 简体中文 | 正體中文 | +/-

You may select the license of your choice.

## Attēlu saites

Attēls ir izmantots šajās lapās:

- Somerseta

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | Canon
Camera model | Canon PowerShot A520
Orientation | Normal
Horizontālā izšķirtspēja | 180 dpi
Vertikālā izšķirtspēja | 180 dpi
File change date and time | 13:13, 6 jūnijā, 2006
Y and C positioning | 1
Exposure time | 1/640 sec (0.0015625)
F Number | f/4
Exif version | 2.2
Date and time of data generation | 13:13, 6 jūnijā, 2006
Date and time of digitizing | 13:13, 6 jūnijā, 2006
Image compression mode | 5
Shutter speed | 9.3125
Aperture | 4
Exposure bias | 0
Maximum land aperture | 2.75
Metering mode | Pattern
Flash | 24
Lens focal length | 5.8125 mm
Color space | sRGB
Focal plane X resolution | 10142.857142857
Focal plane Y resolution | 10142.857142857
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Scene capture type | Standard

Saturs iegūts no "http://lv.wikipedia.org../../../p/e/n/Att%C4%93ls%7EPensford_and_Viaduct.jpg_5b2e.html"

##### Views

- Attēls
- Diskusija
- Pašreizējā versija

##### Meklēt