Attēls:Parallel computer printer port.jpg - Vikipēdija

# Attēls:Parallel computer printer port.jpg

### Vikipēdijas raksts

- Attēls
- Attēla hronoloģija
- Attēlu saites
- Metadata

Size of this preview: 800 × 600 pixel
Image in higher resolution (1787 × 1340 pixel, file size: 504 KB, MIME type: image/jpeg)

Šis fails ir no Wikimedia Commons. Skat. attēla apraksta lapu.

## [edit] Summary

Description | Parellel computer printer port
Source | own work
Date | 2006-05-24
Author | Duncan Lithgow
Permission | Permission is given to use as per the license

## [edit] Licensing

I, the copyright holder of this work, hereby release it into the public domain. This applies worldwide.

In case this is not legally possible:
I grant anyone the right to use this work for any purpose, without any conditions, unless such conditions are required by law.

Afrikaans | Alemannisch | Aragonés | العربية‎ | Български | Català | Česky | Cymraeg | Dansk | Deutsch | Ελληνικά | English | Español | Esperanto | Euskara | فارسی‎ | Français | Galego | 한국어 | हिन्दी | Hrvatski | Ido | Bahasa Indonesia | Íslenska | Italiano | עברית‎ | Kurdî / كوردي | Latina | Lietuvių | Magyar | Bahasa Melayu | Nederlands | Norsk (bokmål) | Norsk (nynorsk) | 日本語 | Polski | Português | Ripoarish | Română | Русский | Shqip | Slovenčina | Slovenščina | Српски | Svenska | ไทย | Türkçe | Українська | Tiếng Việt | Walon | 简体中文 | 繁體中文 | 粵語 | +/-

## Attēlu saites

Attēls ir izmantots šajās lapās:

- Paralēlais ports

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Image title | MINOLTA DIGITAL CAMERA
Camera manufacturer | Minolta Co., Ltd.
Camera model | DiMAGE Z1
Orientation | Normal
Horizontālā izšķirtspēja | 72 dpi
Vertikālā izšķirtspēja | 72 dpi
Software used | Ver. 1.00
File change date and time | 14:49, 24 maijā, 2006
Y and C positioning | 2
Exposure time | 1/100 sec (0.01)
F Number | f/3.2
Exposure Program | Normal program
ISO speed rating | 160
Exif version | 2.2
Date and time of data generation | 14:49, 24 maijā, 2006
Date and time of digitizing | 14:49, 24 maijā, 2006
Image compression mode | 4
Brightness | 3.3
Exposure bias | 0
Maximum land aperture | 3.4
Metering mode | Pattern
Light source | Unknown
Flash | 16
Lens focal length | 13.2 mm
Color space | sRGB
Custom image processing | Custom process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 0
Focal length in 35 mm film | 86
Scene capture type | Standard
Contrast | Normal
Saturation | Normal
Sharpness | Normal
Subject distance range | Macro

Saturs iegūts no "http://lv.wikipedia.org../../../p/a/r/Att%C4%93ls%7EParallel_computer_printer_port.jpg_f0b9.html"

##### Views

- Attēls
- Diskusija
- Pašreizējā versija

##### Meklēt