Attēls:Snoopie.jpg - Vikipēdija

# Attēls:Snoopie.jpg

### Vikipēdijas raksts

- Attēls
- Attēla hronoloģija
- Attēlu saites
- Metadata

No higher resolution available.

Snoopie.jpg‎ (320 × 240 pixel, file size: 65 KB, MIME type: image/jpeg)

snoopie no led

## Attēla hronoloģija

Apzīmējumi: (pašreizējais) = šā attēla pašreizējā versija, (dzēst) = dzēst šo veco versiju, (atjaunot) = nomainīt pret šo veco versiju.
Klikšķini uz datuma, lai aplūkotu tajā datumā augšuplādēto failu..

- (dzēst) (ar pašreizējo) 16:19, 28 oktobrī, 2006 . . Snoopie (Diskusija | devums) . . 320×240 (66 603 baitu) (snoopie no led)

- Izmainīt šo failu ar ārēju programmu

  Skat. instrukcijas Meta-Wiki, lai iegūtu vairāk informācijas.

## Attēlu saites

Nevienā lapā nav norāžu uz šo attēlu.

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | Canon
Camera model | Canon PowerShot A530
File change date and time | 14:54, 19 oktobrī, 2006
Y and C positioning | 1
Exposure time | 1/60 sec (0.016666666666667)
F Number | f/5.5
Exif version | 2.2
Date and time of data generation | 14:54, 19 oktobrī, 2006
Date and time of digitizing | 14:54, 19 oktobrī, 2006
Image compression mode | 5
Shutter speed | 5.90625
Aperture | 4.90625
Exposure bias | 0
Maximum land aperture | 4.90625
Metering mode | Pattern
Flash | 88
Lens focal length | 23.2 mm
Color space | sRGB
Focal plane X resolution | 11520
Focal plane Y resolution | 11571.428571429
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Scene capture type | Standard

Saturs iegūts no "http://lv.wikipedia.org../../../s/n/o/Att%C4%93ls%7ESnoopie.jpg_e7c0.html"

##### Views

- Attēls
- Diskusija
- Pašreizējā versija

##### Meklēt