Imej:Poland Baranow - Castle.jpg - Wikipedia

# Imej:Poland Baranow - Castle.jpg

### Dari Wikipedia bahasa Melayu

- Imej
- Sejarah imej
- Pautan imej
- Metadata

No higher resolution available.

Poland_Baranow_-_Castle.jpg‎ (640 × 427 pixel, file size: 56 KB, MIME type: image/jpeg)

| Fail ini terletak di Wikimedia Commons. Keterangannya di sana ditunjukkan di bawah.

Poland, Baranow Sandomierski - Castle.

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Asturianu | Български | বাংলা | ইমার ঠার | Brezhoneg | Bosanski | Català | Sinugboanong Binisaya | Česky | Dansk | Deutsch | Ελληνικά | English | Esperanto | Español | Eesti | Euskara | فارسی | Suomi | Français | Galego | עברית | Hrvatski | Magyar | Bahasa Indonesia | Ido | Íslenska | Italiano | 日本語 | ქართული | 한국어 | Kurdî / كوردي | Latina | Lëtzebuergesch | Lietuvių | Bahasa Melayu | Nnapulitano | Nederlands | Norsk (nynorsk) | Norsk (bokmål) | Polski | Português | Română | Русский | Slovenčina | Slovenščina | Shqip | Српски | Svenska | తెలుగు | ไทย | Türkçe | Українська | اردو | Tiếng Việt | Volapük | 中文(简体) | 中文(繁體) | +/-

Photo taken by me (Merlin).

## Pautan imej

Halaman-halaman berikut berpaut pada imej ini:

- Poland

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | FUJIFILM
Camera model | MX-2700
Orientation | Normal
Horizontal resolution | 72 dpi
Vertical resolution | 72 dpi
Software used | Digital Camera MX-2700 Ver1.00
File change date and time | 14:05, 10 Ogos 2004
Y and C positioning | 2
F Number | f/8
Exposure Program | Normal program
ISO speed rating | 120
Exif version | 2.1
Date and time of data generation | 14:05, 10 Ogos 2004
Date and time of digitizing | 14:05, 10 Ogos 2004
Image compression mode | 3.2
Shutter speed | 8.4
Aperture | 6
Brightness | 9.1
Exposure bias | 0
Maximum land aperture | 3.4
Metering mode | Pattern
Flash | 0
Lens focal length | 7.6 mm
Color space | sRGB
Focal plane X resolution | 2381
Focal plane Y resolution | 2381
Focal plane resolution unit | 3
Sensing method | One-chip color area sensor

Diperolehi daripada "http://ms.wikipedia.org../../../p/o/l/Imej%7EPoland_Baranow_-_Castle.jpg_ea0c.html"

##### Views

- Imej
- Perbincangan
- Semakan terkini

##### Cari