Image:Emperor Maxentius Louvre Ma3522bis.jpg - Wikipedia

# Image:Emperor Maxentius Louvre Ma3522bis.jpg

### From Wikipedia

- Image
- Historija slike
- Linkovi na sliku
- Metapodaci

Size of this preview: 395 × 600 pixel
Image in higher resolution (1120 × 1700 pixel, file size: 1.15 MB, MIME type: image/jpeg)

| Ova slika je sa Vikimedijinog multimedijalnog skladišta - Commons. Pogledajte stranicu sa opisom.

## [edit] Description

Musée du Louvre, Paris, France
Artist/Maker | Unknown
Description | Bust of Emperor Maxentius (?), Western Roman Emperor from AD 306 to 312. Marble, first half of the 4th century, found at Langres, Champagne, France.
Dimensions | H. 39 cm (15 ¼ in.)
Credit line | From the Tuileries Gardens; in the Louvre collections since 1871
Accession number | Ma 3522 bis
Location | Département des Antiquités grecques, étrusques et romaines, Denon, ground floor, room 29
Photographer/source | Jastrow (2005)

Français : Buste de Maxence (?), empereur d'Occident de 306 à 312. Marbre, première moitié d IVe siècle, découvert à Langres (Champagne, France).

## [edit] Licensing

I, the copyright holder of this work, hereby release it into the public domain. This applies worldwide.

In case this is not legally possible:
I grant anyone the right to use this work for any purpose, without any conditions, unless such conditions are required by law.

Afrikaans | Alemannisch | Aragonés | العربية‎ | Български | Català | Česky | Cymraeg | Dansk | Deutsch | Ελληνικά | English | Español | Esperanto | Euskara | فارسی‎ | Français | Galego | 한국어 | हिन्दी | Hrvatski | Ido | Bahasa Indonesia | Íslenska | Italiano | עברית‎ | Kurdî / كوردي | Latina | Lietuvių | Magyar | Bahasa Melayu | Nederlands | Norsk (bokmål) | Norsk (nynorsk) | 日本語 | Polski | Português | Ripoarish | Română | Русский | Shqip | Slovenčina | Slovenščina | Српски | Svenska | ไทย | Türkçe | Українська | Tiếng Việt | Walon | 简体中文 | 繁體中文 | 粵語 | +/-

## Linkovi na sliku

Sljedeće stranice vode na ovu sliku:

- Pretorijanci

## Metapodaci

Ovaj fajl/datoteka sadržava dodatne podatke koje je vjerojatno dodala digitalna kamera ili skener u procesu snimanja odnosno digitalizacije. Ako je fajl/datoteka mijenjan, podaci možda nisu u skladu sa stvarnim stanjem.

Proizvođač kamere | NIKON CORPORATION
Model kamere | NIKON D70
Orijentacija | Normalno
Vodoravna rezolucija | 300 dpi
Okomita rezolucija | 300 dpi
Korišteni softver | DxO Optics Pro Standard MACOSX 3.55b.6377581.356110 MTF
Datum posljednje promjene fajla | 17:43, 11 decembar-просинац 2005
Razmještaj komponenata Y i C | 2
Ekspozicija | 1/60 sec (0.016666666666667)
F broj dijafragme | f/4
Program ekspozicije | Prioritet dijafragme
ISO vrijednost | 1250
Exif verzija | 2.21
Datum i vrijeme slikanja | 17:43, 11 decembar-просинац 2005
Datum i vrijeme digitalizacije | 17:43, 11 decembar-просинац 2005
Dubina boje poslije sažimanja | 4
Brzina zatvarača | 5.906891
Otvor blende | 4
Kompenzacija ekspozicije | 0
Minimalni broj dijafragme | 2
Režim mjerača vremena | Prosjek sa težištem na sredini
Izvor svjetlosti | Bljeskalica
Bljeskalica | 31
Žarišna daljina leće - Фокусна даљина сочива | 35 mm
Dio sekunde u kojem je slikano | 80
Dio sekunde u kojem je fotografirano | 80
Dio sekunde u kojem je digitalizirano | 80
Prostor boje | sRGB
Tip senzora | Jednokristalni matrični senzor
Dodatna obrada slike | Normalni proces
Režim izbora ekspozicije | Automatski
Balans bijele | Ručno
Razmjer digitalnog zooma | 1
Ekvivalent žarišne daljine za 35 mm film | 52
Tip scene na snimci | Standardno
Kontrast | Normalno
Zasićenje | Normalno
Oštrina | Tvrdo
Raspon udaljenosti subjekata | Nepoznato

Retrieved from "http://sh.wikipedia.org../../../e/m/p/Image%7EEmperor_Maxentius_Louvre_Ma3522bis.jpg_a9e3.html"

##### Views

- Slika
- Rasprava/Разговор
- Trenutna revizija

##### Traži-Тражи