Image:Defibrillator Monitor.jpg - Simple English Wikipedia, the free encyclopedia

# Image:Defibrillator Monitor.jpg

### From Simple English Wikipedia, the free encyclopedia

- Image
- File history
- Links
- Metadata

Size of this preview: 800 × 600 pixel
Image in higher resolution (1600 × 1200 pixel, file size: 702 KB, MIME type: image/jpeg)
This is a file from the Wikimedia Commons, a repository of free content hosted by the Wikimedia Foundation. The description on its description page there and licensing information is visible below.

## [edit] Beschreibung

Description | en: A defibrillator/monitor/pacer from an ambulance in Graz, Austria. For a close-up picture see the link below. de: Ein Defibrillator/Monitor/Schrittmacher aus einem Rettungswagen in Graz, Österreich. In der linken Seitentasche befindet sich eine automatische Blutdruckmanschette und ein Kapnometer, in der mittleren (oberen) Tasche die zwei "Paddles" zum Defibrillieren, sowie ein Tube mit Elektrodengel. In der rechten Seitentasche sind die Kabel für die (bis zu 12-kanalige) EKG-Überwachung und Pulsoxymetrie, sowie die EKG-Elektroden untergebracht. Das Gerät ist weiterhin in der Lage, einen externen Schrittmacher zu betreiben, sowie eine invasive Blutdruckmessung durchzuführen. In der Mitte unten befindet sich der Monitor, jeweils seitlich davon die verschiedenen Bedienelemente. Für eine Nahansicht, siehe Link weiter unten ("other versions").
Source | own photo
Date | created 19. Feb. 2006
Author | Ernstl
Permission | CC-BY-SE-2.5
Other versions | Closeup

## [edit] Licensing

I, the author of this work, hereby publish it under the following license:

| This file is licensed under the Creative Commons Attribution ShareAlike 2.5 License. In short: you are free to share and make derivative works of the file under the conditions that you appropriately attribute it, and that you distribute it only under a license identical to this one. Official license

## Links

The following pages link to this file:

- Defibrillator

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Image title | KONICA MINOLTA DIGITAL CAMERA
Camera manufacturer | Konica Minolta Camera, Inc.
Camera model | DiMAGE Xg
Orientation | Normal
Horizontal resolution | 72 dpi
Vertical resolution | 72 dpi
Software used | DiMAGE Xg Ver1.02
File change date and time | 11:22, 19 February 2006
Y and C positioning | 2
Exposure time | 1/8 sec (0.125)
F Number | f/2.8
Exposure Program | Normal program
ISO speed rating | 100
Exif version | 2.2
Date and time of data generation | 11:22, 19 February 2006
Date and time of digitizing | 11:22, 19 February 2006
Image compression mode | 4
Brightness | 0.1
Exposure bias | 0
Maximum land aperture | 3
Metering mode | Pattern
Light source | Unknown
Flash | 16
Lens focal length | 6 mm
Color space | sRGB
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 0
Focal length in 35 mm film | 38
Scene capture type | Standard
Contrast | Normal
Saturation | Normal
Sharpness | Normal
Subject distance range | Close view

Retrieved from "http://simple.wikipedia.org../../../d/e/f/Image%7EDefibrillator_Monitor.jpg_1a20.html"

##### Views

- File
- Talk
- Newest version

##### Search