Mékanika taneuh - Wikipédia

# Mékanika taneuh

### Ti Wikipédia, énsiklopédi bébas

Mekanika taneuh nyaeta hiji widang elmu nu migunakeun prinsil mekanika teknik keur ngira-ngira sipat mekanik taneuh. Karl von Terzaghi, nu ngamimitian migunakeun prinsip rasional dina widang rekayasa taneuh, disebut salaku Bapak Mekanika Taneuh.

Mekanika taneuh ngarupakeun salah sahiji disiplin penting tina sababaraha cabang rekayasa, saperti Rékayasa sipil, Rekayasa geoteknik sarta Geologi rekayasa. Mekanika taneuh dipake dina desain pondasi keur ngadukung struktur, tanggul, tembok panahan, earthwork sarta wangunan bawah taneuh.

Perkolasi cai ngaliwatan taneuh hal penting dina konstruksi torowongan sarta pondasi jero, sarta wangunan nu pakait jeung cai saperti pilar jembatan jeung waduk.

## [édit] Karakter Dasar Taneuh

Taneuh diwangun ku 3 komponen: udara, cai, jeung padet. Padet nyaeta partikel nu diwangun tina ukuran parikel lempung saperti lebu nepi ka bongkah gede. Lobana cai jeung udara dina jero sampel taneuh ngarupakeun faktor nu nangtukeun pasipatan taneuh. Hal sejenna nu mangaruhan kana sipat taneuh nyaeta tipe partikel nu nyusunna.

## [édit] Rembesan

Rembesan nyaeta ngalirna fluida ngaliwatan pori taneuh, boh ka luhur atawa ka handap. Rembesan sahandapeun waduk sarta jajaran pile biasana diitung make grafik konstruksi sederhana saperti flownet. Lamun kecepatan rembesan cukup gede, bakal kajadian erosi taneuh.Erosi taneuh ieu mangrupa hal nu gede pangaruhna lamun wangunan nu dijieun aya di tempat nu niley luhur cai taneuh kacida beda ti hiji tempat ka tempat sejenna. Kajadin erosi dina jero taneuh ieu oge disebut "piping", nu bisa mangaruhan kana runtuhna hiji wangunan, sarta hal nu ilahar nyababkeun runtuhna waduk. Rembesa ka arah luhur ngurangan efektif stress partikel taneuh. Dina kasus beda luhur cai taneuh sarua atawa leuwih gede tina niley kritisna, mangka efektif stress bakal turun ngadeukeutan enol. Kaayaan siga kieu disebutna kaayaan "quicksand" atawa "boiling".

## [édit] Efektif Stress σ '

Konsep efektif stress ngarupakeun hal nu penting keur ngarti kana sifat cai dina kaayaan anu beda-beda. Efektif stress nyaeta ukuran gedena beban nu ditahan ku awak taneuh. Ukuran ieu ngagambarkeun kamampu taneuh keur nahan kuat geser. Lamun efektif stress taneuh deukeut ka angka nol, kaayaan quick bakal kajaadian (tempo quicksand).

Efektif stess (σ ' ) taneuh diitung tina dua parameter hasil tina panalungtikan nyaeta , total stress (σ) jeung pore water pressure (μ) saperti ieu:

  σ' = σ - μ

dimana satuan kabehanna nyaeta tekanan.

### [édit] Total Stress σ

Total stress σ sarua jeung overburden pressure, nyaeta beurat barang dina kaayaan cicing saluhureun taneuh, kaasup oge taneuh nu di luhurna. Total stress teu salawasna nambahan sanajan beuki ka jero taneuh.

### [édit] Pore water pressure μ

Pore water pressure μ bisa diitung salaku hydrostatic pressure cai dumasar kana fluid statics lamun ieu dianggap yen aliran cai ngaliwatan taneuh kacida launna. Anggapan ieu bener keur kayaan nu ilahar (iwal ti dina kaayaan quick condition ). Pore water pressure bisa diperkirakeun sarua jeung nol saluhureun beungeut cai taneuh sarta nambahan sacara linier ku nambahna jero taneuh sahandapeun "water table".

## [édit] Kuat geser

Kuat geser nyaeta kakuatan nahan taneuh maximum saacan kajadian shear failure sapanjang bidang specific failure . Kuat geser taneuh pakait raket jeung tipe taneuh, mangka, respons taneuh granular keur beban taneuh gumantung kana gedena density taneuh sorangan, numana cohesive overconsolidated taneuh nembongkeun kayaan nu beda. Kuat geser taneuh dipangaruhan ku:(i) katahanan friksi antara partikel taneuh jeung tempat dimana aya kontak, (ii) kohesi antar partikel sarta (iii) interlocking antar partikel. Hukum failure keur taneuh: T=c+[(Pn)(Tan O)] numana: T: Kuat geser. c: Kohesi ( sarua jeung nol keur nu teu mibanda kohesi). Pn: Normal Stress O : Sudut geser dalam

## [édit] Teori Kondolidasi

Lamun aliran cai nu asup atawa kaluar tina taneuh henteu nyababkeun robahna volume taneuh, mangka ieu aliran disebutseepage. Sabalikna, lamun aliran cai nu asup atawa kaluar tina taneuh nyababkeun robahna volume taneuh disebutna transient. Proses robahna volume taneuh akibat ayana aliran transient ieu disebut konsolidasi. Hal ieu pakait jeung robahna efektif stress dina matriks taneuh ku ayana surface loading (atawa unloading) atawa variasi dina posisi beungeut cai taneuh. Excess porewater pressure (upamana load-induced porewater pressure) bisa kajadian dina dua kasus diluhur tadi, salian ti eta bisa oge kajadian dina waktu kaluarna cai tina masa taneuh sacara ngadadak (positive pore water pressure) atawa sabalikna (negative porewater pressure). Aliran cai ieu kontinyu dina changing rate salila sakabeh excess pressure kaluar, sarta saruana tekanan nu aya dumasar kana prinsip tekanan efektif.

Dumasar sajarah geologi, lamun taneuh dumasar kana kajadian unloading, upamana leungitna es nu nutupan taneuh atawa ku kajadian erosi, maka tekanan taneuh nu aya ayeuna ngarupakeun overburden pressure (beurat taneuh sorangan) bakal leuwih leutik tinimbang nu aya samemeh proses unloading, sarta taneuh ieu disebut overconsolidated. Sejenna, lamun taneuh henteu dumasar kana kajadian unloading dina sajarah geologi-na, mangka overburden pressure ayeuna, ngarupakeun tekanan panggedena dina sajarahna, mangka ieu taneuh disebutna normally consolidated.

## [édit] Kastabilan lereng

An exposed ground surface that makes any angle other than horizontal is called an unrestrained slope. If gravity is large enough, failure of the slope can occur. Analysis of slopes is difficult and tedious to perform. Engineers wishing to perform this analysis must determine the factor of safety of the slope. This factor of safety is a function of the soil properties, angle of repose, climate, and vegetation, as well as many other factors.

In order to find the factor of safety of soil, one must first find the critical equillibrium, or loading to the precipice of the slope failing. Once this equillibrium is found, a factor of safety can be calculated based on typical loadings that can be expected.

## [édit] Panalungtikan taneuh

Panalungtikan taneuh ngarupakeun hal penting dina raraga ngumpulkeun informasi ngeunaan tanueh keur kaperluan perencanaan, disain tur konstruksi proyek anyar. Panalungtikan taneuh kabagi dua tahapan nyaeta primer jeung sekunder. Panalungtikan primer ilaharna dimimitian saacan konstruksi sarta gumantung kana sifat alami proyek. Kagiatanna kaasup survey permukaan (survey topografi, perkiraan volume galian, kemiringan keur drainasi), sarta panalungtikan handapeun taneuh (posisi beungeut cai taneuh, tipe taneuh, jero taneuh keur bearing capacity, sipat taneuh). Panalungtikan sekunder ilaharna dipigawe salila proyek lumangsung sarta keur kaperluan akses, kaayaan jeung kaamanan proyek.

## [édit] Rujukan

- Azizi, F., Applied Analyses in Geotechnics, (2000), E & FN SPON.
- Terzaghi, K., 1943, Theoretical Soil Mechanics, John Wiley and Sons, New York
- Craig, R.F., 1974, Soil Mechanics, Spon Press, London
- Wikipedia Basa Inggris, Juli 2006.

## [édit] Tempo oge

- Perméabilitas (géologi)
- Hidrogéologi (aquifer characteristics closely related to soil characteristics)
- Rékayasa géotéhnik

Disalin ti "http://su.wikipedia.org../../../m/%C3%A9/k/M%C3%A9kanika_taneuh.html"

Kategori: Rékayasa wangunan | Rékayasa sipil | Mékanika taneuh

##### Views

- Artikel
- Sawala
- Révisi kiwari

##### Sungsi

##### Basa séjén

- Deutsch
- English
- Tiếng Việt
- 中文