Gambar:Cgk domestic terminalJPG.jpg - Wikipédia

# Gambar:Cgk domestic terminalJPG.jpg

### Ti Wikipédia, énsiklopédi bébas

- Gambar
- Jujutan gambar
- Tumbu gambar
- Metadata

Size of this preview: 800 × 249 pixel
Image in higher resolution (1660 × 517 pixel, file size: 135 KB, MIME type: image/jpeg)

| Koropak ieu asalna ti Wikimedia Commons. Tempo kaca dadaranana pikeun leuwih jéntré.

Soekarno-Hatta International Airport Terminal I in Cengkareng, Indonesia. Taken from Wikipedia Nederlands

Author: w:nl:Gebruiker:Hullie

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Asturianu | Български | বাংলা | ইমার ঠার | Brezhoneg | Bosanski | Català | Sinugboanong Binisaya | Česky | Dansk | Deutsch | Ελληνικά | English | Esperanto | Español | Eesti | Euskara | فارسی | Suomi | Français | Galego | עברית | Hrvatski | Magyar | Bahasa Indonesia | Ido | Íslenska | Italiano | 日本語 | ქართული | 한국어 | Kurdî / كوردي | Latina | Lëtzebuergesch | Lietuvių | Bahasa Melayu | Nnapulitano | Nederlands | Norsk (nynorsk) | Norsk (bokmål) | Polski | Português | Română | Русский | Slovenčina | Slovenščina | Shqip | Српски | Svenska | తెలుగు | ไทย | Türkçe | Українська | اردو | Tiếng Việt | Volapük | 中文(简体) | 中文(繁體) | +/-

## Tumbu gambar

Kaca nu numbu ka gambar ieu:

- Bandara Soekarno-Hatta

## Metadata

Ieu koropak ngandung émbaran tambahan, nu sigana asalna tina kaméra digital atawa paminday nu dipaké pikeun ngadigitalkeunana. Mun ieu koropak geus dirobah tina bentuk aslina, datana bisa jadi teu bener.

Camera manufacturer | Canon
Camera model | Canon DIGITAL IXUS v3
Orientation | Normal
Résolusi horizontal | 180 dpi
Vertical resolution | 180 dpi
Wanci jeung titimangsa parobahan koropak | 19:00, 10 Juli 2005
Y and C positioning | 1
Exposure time | 1/500 sec (0.002)
F Number | f/2.8
Exif version | 2.2
Titimangsa jeung wanci dijieunna data | 10:43, 10 Désémber 2004
Titimangsa jeung wanci digitisasi | 10:43, 10 Désémber 2004
Mode komprési gambar | 3
Shutter speed | 8.96875
Aperture | 2.96875
Exposure bias | 0
Maximum land aperture | 2.96875
Metering mode | Pattern
Flash | 24
Lens focal length | 5.40625 mm
Color space | sRGB
Focal plane X resolution | 9893.7198067633
Focal plane Y resolution | 9846.1538461538
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor
Custom image processing | Prosés normal
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Scene capture type | Standard

Disalin ti "http://su.wikipedia.org../../../c/g/k/Gambar%7ECgk_domestic_terminalJPG.jpg_b814.html"

##### Views

- Gambar
- Sawala
- Révisi kiwari

##### Sungsi