Image:Speyer Dom Laengsseite.jpg - Wikipedia, déi fräi Enzyklopedie

# Image:Speyer Dom Laengsseite.jpg

### Vu Wikipedia, der fräier Enzyklopedie.

- Image
- Historique vum Bild
- Biller Links
- Metadata

Bild an héijer Opléisung eroflueden (998x489, 112 KB)

| Dëse Fichier gouf automatesch vu Wikimedia Commons importéiert. Fir ze wëssen wéi een e Bild vu Commons importéiert, kuckt w.e.g. : Wikipedia:Wikimedia Commons. Kuckt och d'Deskriptiounssäit vun dësem Bild fir méi Informatiounen zum Auteur an zur Lizenz.

La bildo estas kopiita de wikipedia:de. La originala priskribo estas:

- Beschreibung: Speyerer Dom
- Quelle: fotografiert am 4. Juli 2004
- Fotograf: Stefan Kühn
- Copyright Status: GNU-FDL Freie Dokumentationslizenz

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Česky | Deutsch | English | Español | Français | Italiano | 日本語 | 한국어 | Nederlands | Polski | Português | Slovenčina | Svenska | עברית +/-

date/time | username | edit summary
--- | --- | ---
09:40, 5. Jan 2005 | de:Benutzer:Stefan Kühn |
19:46, 6. Jul 2004 | de:Benutzer:Stefan Kühn |
19:44, 6. Jul 2004 | de:Benutzer:Stefan Kühn | (Speyer_Dom_Laengsseite)

## Biller Links

Folgend Säite linken op dëst Bild:

- Rheinland-Pfalz

## Metadata

Dëse Fichier enthält weider Informatiounen (EXIF-Metadaten), déi am Prinzip vun der Digitalkamera oder dem Scanner komme mat deem de Fichier geschafe gouf. Duerch nodréilecht Beschaffe vum Originalfichier kënnen e puer Donnéeë verännert gi sinn, déi dann net méi onbedéngt der Realitéit entspriechen.

Image title | MINOLTA DIGITAL CAMERA
Camera manufacturer | Minolta Co., Ltd.
Camera model | DiMAGE Z1
Orientation | Normal
Horizontal resolution | 72 dpi
Vertical resolution | 72 dpi
Software used | Ver. 1.00
File change date and time | 14:06, 4 Juli 2004
Y and C positioning | 2
Exposure time | 1/400 sec (0.0025)
F Number | f/5.6
Exposure Program | Normal program
ISO speed rating | 50
Exif version | 2.2
Date and time of data generation | 14:06, 4 Juli 2004
Date and time of digitizing | 14:06, 4 Juli 2004
Image compression mode | 4
Brightness | 8
Exposure bias | 0
Maximum land aperture | 3.6
Metering mode | Pattern
Light source | Unknown
Flash | 16
Lens focal length | 26.3 mm
Color space | sRGB
Custom image processing | Custom process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 0
Focal length in 35 mm film | 172
Scene capture type | Standard
Contrast | Normal
Saturation | Normal
Sharpness | Normal
Subject distance range | Distant view

Vun "http://lb.wikipedia.org../../../s/p/e/Image%7ESpeyer_Dom_Laengsseite.jpg_fbc5.html"

##### Views

- Bild
- Diskussioun
- Aktuell Revisiounen

##### Sichen