Figura:LCD layers.svg - Wikipedia

# Figura:LCD layers.svg

### Nga Wikipedia, Enciklopedia e Lirë

- Figura
- Historia e skedës
- Lidhje skedash

LCD_layers.svg‎ (13KB, lloji MIME: `image/svg+xml`)

| Kjo skedë ndodhet tek projekti Wikimedia Commons. Ju lutem shikoni faqen përshkruese që ndodhet atje.

Reflective twisted nematic w:liquid crystal display.

1. Vertical filter film to polarize the light as it enters.
2. Glass substrate with ITO electrodes. The shapes of these electrodes will determine the dark shapes that will appear when the LCD is turned on. Vertical ridges are etched on the surface so the liquid crystals are in line with the polarized light.
3. Twisted nematic liquid crystals.
4. Glass substrate with common electrode film (ITO) with horizontal ridges to line up with the horizontal filter.
5. Horizontal filter film to block/allow through light.
6. Reflective surface to send light back to viewer.

Original artwork by ed g2s • talk.

I, the author of this work, hereby publish it under the following licenses:

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Česky | Deutsch | English | Español | Français | Italiano | 日本語 | 한국어 | Nederlands | Polski | Português | Slovenčina | Svenska | עברית +/-

| This file is licensed under the Creative Commons Attribution ShareAlike license versions 2.5, 2.0, and 1.0

You may select the license of your choice.

## Lidhje skedash

Këto faqe lidhen tek kjo skedë:

- LCD

Marrë nga "http://sq.wikipedia.org../../../l/c/d/Figura%7ELCD_layers.svg_74db.html"

##### Views

- Figura
- Diskutimet
- Versioni i tanishëm

##### Kërko