Beeld:LakeErie-2.jpg - Wikipedia

# Beeld:LakeErie-2.jpg

### vanuit Wikipedia, die vrye ensiklopedie.

- Beeld
- Prentgeskiedenis
- Prentskakels
- Metadata

LakeErie-2.jpg‎ (160KB, MIME type: `image/jpeg`)

Hierdie is 'n bydrae vanuit die Wikimedia Commons, 'n versameling vrye inhoud wat deur die Wikimedia Foundation ondersteun en gedra word. Sien die ooreenstemmende beskrywingsblad op die Commons vir meer inligting oor hierdie spesifieke bydrae.

Source: Photo by User:GandZ

I, the author of this work, hereby publish it under the following license:

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Deutsch | English | Español | Français | Italiano | 日本語 | 한국어 | Nederlands | Polski | Português | Slovenčina | Svenska | עברית +/-

Lake Erie (frozen) from Cleveland Ohio. 18/Jan/2003 by Kodak DC280.

## Prentskakels

Die volgende bladsye gebruik hierdie prent:

- Groot Mere

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | EASTMAN KODAK COMPANY
Camera model | KODAK DC280 ZOOM DIGITAL CAMERA
Orientation | Normal
Horizontal resolution | 192 dpi
Vertical resolution | 192 dpi
Y and C positioning | 1
Copyright holder | KODAK DC280 ZOOM DIGITAL CAMERA
Exposure time | 1/360 sec (0.0027777777777778)
F Number | f/8
Exif version | 2.1
Date and time of data generation | 15:58, 18 Januarie 2003
Date and time of digitizing | 15:58, 18 Januarie 2003
Shutter speed | 8.5
Aperture | 6
Exposure bias | 0
Maximum land aperture | 3.1
Metering mode | Average
Light source | Daylight
Flash | 0
Lens focal length | 6.3 mm
Color space | sRGB
Exposure index | 80
Sensing method | One-chip color area sensor

Ontsluit van "http://af.wikipedia.org../../../l/a/k/Beeld%7ELakeErie-2.jpg_4262.html"

##### Views

- Beeld
- Bespreking
- Huidige wysiging

##### Soek