Image:Bruxelles-Luxembourg.jpg - Wikipedia, déi fräi Enzyklopedie

# Image:Bruxelles-Luxembourg.jpg

### Vu Wikipedia, der fräier Enzyklopedie.

- Image
- Historique vum Bild
- Biller Links
- Metadata

Bruxelles-Luxembourg.jpg‎ (51KB, MIME type: `image/jpeg`)

| Dëse Fichier gouf automatesch vu Wikimedia Commons importéiert. Fir ze wëssen wéi een e Bild vu Commons importéiert, kuckt w.e.g. : Wikipedia:Wikimedia Commons. Kuckt och d'Deskriptiounssäit vun dësem Bild fir méi Informatiounen zum Auteur an zur Lizenz.

## [edit] Summary

Description | Bruxelles-Luxembourg/Brussel-Luxemburg railway station, old building
Source | French language wikipedia
Date | 22 March 2004
Author | fr:Utilisateur:BenoitL
Permission | GFDL

## [edit] Licensing

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Deutsch | English | Español | Français | Italiano | 日本語 | 한국어 | Nederlands | Polski | Português | Slovenčina | Svenska | עברית +/-

## Biller Links

Folgend Säite linken op dëst Bild:

- Gare de Bruxelles-Luxembourg

## Metadata

Dëse Fichier enthält weider Informatiounen (EXIF-Metadaten), déi am Prinzip vun der Digitalkamera oder dem Scanner komme mat deem de Fichier geschafe gouf. Duerch nodréilecht Beschaffe vum Originalfichier kënnen e puer Donnéeë verännert gi sinn, déi dann net méi onbedéngt der Realitéit entspriechen.

Camera manufacturer | Canon
Camera model | Canon PowerShot A40
Orientation | Normal
Horizontal resolution | 180 dpi
Vertical resolution | 180 dpi
File change date and time | 13:05, 22 Mäerz 2004
Y and C positioning | 1
Exposure time | 1/800 sec (0.00125)
F Number | f/3.5
Exif version | 2.2
Date and time of data generation | 13:05, 22 Mäerz 2004
Date and time of digitizing | 13:05, 22 Mäerz 2004
Image compression mode | 3
Shutter speed | 9.65625
Aperture | 3.6147155761719
Exposure bias | 0
Maximum land aperture | 2.9708557128906
Metering mode | Pattern
Flash | 24
Lens focal length | 7.84375 mm
Color space | sRGB
Focal plane X resolution | 7766.9902912621
Focal plane Y resolution | 7741.935483871
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Scene capture type | Standard

Vun "http://lb.wikipedia.org../../../b/r/u/Image%7EBruxelles-Luxembourg.jpg_0c70.html"

##### Views

- Bild
- Diskussioun
- Aktuell Revisiounen

##### Sichen