Fil:N64-cartridge-chip side-wo heatsink.jpg - Wikipedia

# Fil:N64-cartridge-chip side-wo heatsink.jpg

### Frå Wikipedia – det frie oppslagsverket

- Fil
- Filhistorikk
- Fillenkjer
- Metadata

Last ned høgoppløysingsversjon (1269x1140, 324 KB)

| Dette er ei fil frå Wikimedia Commons. Sjå filomtalen der for meir informasjon.

Følgjande er henta frå filomtalen åt denne fila på Wikimedia Commons:

This is the standard style and color cartridge of the N64 console gaming system taken apart. Photo is of the chip itself resting in one side of the cartridge. When I first saw it I thought about how much of the cartridge is AIR. I guess they just did that for a better grip and to make the customer feel like he was buying more than just a circuit board with 3 small chips on it. Of course, he was just buying the game ON the chips and not the chips themselves.

- Author: mboverload
- Date: Taken and uploaded on 2/25/2005

| This image has been released into the public domain by its author, mboverload. This applies worldwide. In some countries this may not be legally possible; if so: mboverload grants anyone the right to use this work for any purpose, without any conditions, unless such conditions are required by law.

## Fillenkjer

Dei følgjande sidene har lenkjer til denne fila:

- Spelekassett

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Kameraprodusent | Hewlett-Packard
Kameramodell | HP PhotoSmart 318
Oppløysing i breidda | 72 dpi
Oppløysing i høgda | 72 dpi
Programvare brukt | V4.00
Y- og C-posisjon | 2
Eksponeringstid | 126807/500000 sec (0.253614)
F-nummer | f/28
Lysfølsemd (ISO) | 100
Exif-versjon | 1.2
Dato og tid laga | 02:14, 24 februar 2005
Dato og tid digitalisert | 02:14, 24 februar 2005
Image compression mode | 0.07
Lukkarfart | 1.97
Blendartal | 3
Exposure bias | 0
Maximum land aperture | 6
Motivavstand | 0.2 meter
Lysmålarmodus | Snittmåling med vekt på midten
Blits | 0
Linsefokallengd | 6.79 mm
Fargerom | sRGB

Henta frå «http://nn.wikipedia.org../../../n/6/4/Fil%7EN64-cartridge-chip_side-wo_heatsink.jpg_7afc.html»

##### Views

- Fil
- Diskusjon
- Noverande versjon

##### Søk