Image:1950's television.jpg - Wikipedia

# Image:1950's television.jpg

### From Wikipedia

- Image
- File history
- Links
- Metadata

Download high resolution version (1024x768, 97 KB)

| Ova slika je sa Vikimedijinog multimedijalnog skladišta - Commons. Pogledajte stranicu sa opisom.

Photo: Zaphod

Permission is granted to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License".

العربية | Deutsch | English | Español | Français | Italiano | 日本語 | 한국어 | Nederlands | Polski | Português | Slovenčina | Svenska | עברית +/-

## Links

The following pages link to this file:

- Televizija

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | Canon
Camera model | Canon DIGITAL IXUS 430
Orientation | Normal
Horizontal resolution | 180 dpi
Vertical resolution | 180 dpi
Software used | ACD Systems Digital Imaging
File change date and time | 20:11, 6 februar-вељача 2005
Y and C positioning | 1
Exposure time | 1/8 sec (0.125)
F Number | f/2.8
Exif version | 2.1
Date and time of data generation | 16:02, 6 februar-вељача 2005
Date and time of digitizing | 16:02, 6 februar-вељача 2005
Image compression mode | 3
Shutter speed | 3
Aperture | 2.96875
Exposure bias | 0
Maximum land aperture | 2.96875
Metering mode | Pattern
Flash | 16
Lens focal length | 7.40625 mm
DateTime subseconds | 485
Color space | sRGB
Focal plane X resolution | 3657.1428571429
Focal plane Y resolution | 3657.1428571429
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Scene capture type | Standard

Retrieved from "http://sh.wikipedia.org../../../1/9/5/Image%7E1950%27s_television.jpg.html"

##### Views

- File
- Rasprava/Разговор
- Trenutna revizija

##### Traži-Тражи