Gambar:Yamajr.JPG - Wikipédia

# Gambar:Yamajr.JPG

### Ti Wikipédia, énsiklopédi bébas

- Gambar
- Jujutan gambar
- Tumbu gambar
- Metadata

Buka vérsi résolusi alus (2048x1536, 813 KB)

| Koropak ieu asalna ti Wikimedia Commons. Tempo kaca dadaranana pikeun leuwih jéntré.

## [edit] Summary

Description | JR Yamanote line train
Source | english wikipedia, uploaded on 11. Jan. 2005 by en:User:Xavier2000
Date | May 2004
Author | Richard Brown
Permission | released under GFDL in en.wikipedia

## [edit] Licensing

Xavier2000 on the English Wikipedia project has granted permission to copy, distribute and/or modify this document under the terms of the GNU Free Documentation License, Version 1.2 or any later version published by the Free Software Foundation; with no Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A copy of the license is included in the section entitled "GNU Free Documentation License."
Subject to disclaimers.

## Tumbu gambar

Kaca nu numbu ka gambar ieu:

- Tokyo

## Metadata

Ieu koropak ngandung émbaran tambahan, nu sigana asalna tina kaméra digital atawa paminday nu dipaké pikeun ngadigitalkeunana. Mun ieu koropak geus dirobah tina bentuk aslina, datana bisa jadi teu bener.

Camera manufacturer | FUJIFILM
Camera model | FinePix S5000
Orientation | Normal
Résolusi horizontal | 72 dpi
Vertical resolution | 72 dpi
Software used | Digital Camera FinePix S5000 Ver3.00
Wanci jeung titimangsa parobahan koropak | 01:05, 22 Méi 2004
Y and C positioning | 2
Exposure time | 1/240 sec (0.0041666666666667)
F Number | f/3.2
Exposure Program | Normal program
ISO speed rating | 200
Exif version | 2.2
Titimangsa jeung wanci dijieunna data | 01:05, 22 Méi 2004
Titimangsa jeung wanci digitisasi | 01:05, 22 Méi 2004
Mode komprési gambar | 2
Shutter speed | 7.9
Aperture | 3.4
Brightness | 5.19
Exposure bias | 0
Maximum land aperture | 3
Metering mode | Pattern
Light source | Unknown
Flash | 16
Lens focal length | 17.2 mm
Color space | sRGB
Focal plane X resolution | 3827
Focal plane Y resolution | 3827
Focal plane resolution unit | 3
Sensing method | One-chip color area sensor
Custom image processing | Prosés normal
Exposure mode | Auto exposure
White Balance | Auto white balance
Scene capture type | Standard
Sharpness | 3
Subject distance range | Unknown

Disalin ti "http://su.wikipedia.org../../../y/a/m/Gambar%7EYamajr.JPG_dadf.html"

##### Views

- Gambar
- Sawala
- Révisi kiwari

##### Sungsi