ISO 3166-2 - วิกิพีเดีย

# ISO 3166-2

### จากวิกิพีเดีย สารานุกรมเสรี

รหัสมาตรฐาน ISO 3166-2 คือส่วนที่ 2 ของมาตรฐาน ISO 3166 อธิบายถึงตำแหน่งส่วนการปกครองต่างๆ ในแต่ละประเทศ หรือเขตการปกครองอิสระ จุดประสงค์ของการสร้างมาตรฐานเพื่อใช้เป็นคำย่อขนาดสั้น สำหรับสถานที่ ใช้ทั่วโลก ในปัจจุบันมีรหัสทั้ง 3700 รหัส ตัวอย่างรหัสได้แก่ เช่น จังหวัดศรีสะเกษ คือ รหัส TH-33 สำหรับรหัสในแต่ละประเทศ ดูที่ ISO 3166-1 (รหัสประเทศ) โดยจะมีรหัสใกล้เคียงกับรหัสอินเทอร์เน็ตของแต่ละประเทศ

## [แก้] รูปแบบ

รหัส ISO 3166-2 ประกอบด้วยสองส่วนโดยแย่งแยกด้วยเครื่องหมาย"ขีด" โดยส่วนแรกคือ ISO 3166-1 alpha-2 และส่วนหลังคือ ตัวอักษรหรือตัวเรก 2 หรือ 3 หลัก โดยส่วนหลังมักจะอ้างอิงตามรหัสประเทศ

## [แก้] การเปลี่ยนแปลง

การเปลี่ยนแปลงในระบบ ISO 3166-2 มีทั้งหมด 6 ครั้ง ในจดหมายข่าวดังนี้

1. ISO 3166-2:2000-06-21
2. ISO 3166-2:2002-05-21
3. ISO 3166-2:2002-08-20
4. ISO 3166-2:2002-12-10
5. ISO 3166-2:2003-09-05
6. ISO 3166-2:2004-03-08

## [แก้] Format matrix with links to codes

รหัสบางส่วนพัฒนาโดย ISO 3166/MA เป็นรหัสที่มีการจดลิขสิทธิ์ไว้ ซึ่งมีการใช้ในบางประเทศ

ความยาว | alpha | ตัวเลข | alpha-numeric
--- | --- | --- | ---
constant 1 char | Free: Partially free: ISO - Copyright: Unsorted: AR, BO, CR, EC, FJ, GM, KI, KM, LS, LU, MG, NE, RW, SL, ST, TG, TM, VE | GA, IS, AT | PA
constant 2 chars | Free: CH, US Partially free: AL, ID ISO - Copyright: Unsorted: AE, AM, BI, BJ, BN, BR, BS, BW, BY, CA, CD, CF, CL, CM, CV, CZ, DE, DJ, ER, ET, FI, GE, GH, GN, GT, GW, GY, HN, HT, HU, IN, IT, IQ, JO, KW, LA, LB, LR, LT, LV, LY, MD, MU, MW, NA, NG, NI, NL, NP, OM, PK, PL, QA, SB, SH, SK, SN, SO, SR, SV, SY, SZ, TJ, TL, UY, UZ, WS, YE, YU, ZA, ZW | Free: Partially free: TN ISO - Copyright: Unsorted: BD, BG, BH, CI, CN, CU, CY, DO, DZ, EE, GR, HR, IR, JM, JP, KR, LK, MM, MY, NO, PT, SA, SD, TR, TZ, UA, UM, VN, ZM | Free: FR Unsorted: BT
constant 3 chars | Free: Partially free: KP ISO - Copyright: MA Unsorted: AO, AF, BA, BE, BF, CS, FM, GB, KZ, MD, MH, MX, NZ, PE, PG, PH, TT, TW | Free: Partially free: ISO - Copyright: Unsorted: DK, KE, SI, UG, VU |

mixed
1,2 chars

Free: IE

Partially free:
ISO - Copyright:
Unsorted: no system?: ES, GQ, IL
1 for regions, 2 for capital: KG
1 for capital, 2 for departments: RO
1 as the general rule, 2 for exceptions SE

Free:
Partially free:
ISO - Copyright:
Unsorted: KH

Free:
Partially free:
ISO - Copyright:
Unsorted: TH

mixed
2,3

Free:
Partially free:
ISO - Copyright: CO
Unsorted: ?:AU, BZ, EG, TD
2 for republics, 3 for cities, regions, districts: RU
2 for cities, 3 for rayons: AZ
2 for capital, 3 other: ??

MR, MV

mixed 1,3 | Free: Partially free: ISO - Copyright: Unsorted: MZ | Free: Partially free: ISO - Copyright: Unsorted: MN | Free: Partially free: ISO - Copyright: Unsorted: ML
mixed 1,2,3 |  |  | Free: Partially free: ISO - Copyright: Unsorted:CG, PY

## [แก้] ดูเพิ่ม

- ISO 3166-1

## [แก้] เว็บไซต์อื่น

- http://www.iso.org/iso/en/prods-services/iso3166ma/03updates-on-iso-3166/iso_3166-2_track.html
- http://www.iso.org/iso/en/prods-services/iso3166ma/04background-on-iso-3166/iso3166-2.html
- http://www.unece.org/cefact/locode/service/sublocat.htm
- http://geotags.com/iso3166/

ดึงข้อมูลจาก "http://th.wikipedia.org../../../i/s/o/ISO_3166-2_5396.html".

หมวดหมู่: มาตรฐานสากล

##### Views

- บทความ
- อภิปราย
- รุ่นปัจจุบัน

##### ค้นหา

##### ภาษาอื่น

- Alemannisch
- Asturianu
- Български
- Català
- Česky
- Dansk
- Deutsch
- English
- Esperanto
- Español
- Euskara
- Français
- Magyar
- Bahasa Indonesia
- Italiano
- 日本語
- Latina
- Lietuvių
- Nederlands
- Norsk (bokmål)
- Polski
- Português
- Română
- Slovenčina
- Svenska
- Tiếng Việt
- 中文