Wêne:Derwês Serhedî.jpg - Wîkîpediya

# Wêne:Derwês Serhedî.jpg

### Ji Wîkîpediya

- Wêne
- Dîroka datayê
- Lînkên vî wêneyî
- Metadata

Versyonekî jê mezintir tune.
Derwês_Serhedî.jpg (292 × 407 pixel, mezinbûnê data: 101 KB, MIME-typ: image/jpeg)

| Ev wêne di bin lîsansa Creative Commons Attribution ShareAlike License v. 2.5 de ye.

## Dîroka datayê

Li demekê xwe, manê tu kanibê verzîyona data di wê demê da bibînê.

| Roj / Katjimêr | Bikarhêner | Mezinbûn | Mezinbûna data'yê | Nivîs
(niha) | 22:32, 7 rêbendan 2007 | Metin Can (Nîqaş | Beşdarî) | 292 x 407 | 101 KB |
| 22:26, 7 rêbendan 2007 | Metin Can (Nîqaş | Beşdarî) | 800 x 797 | 691 KB | Reverted to earlier revision
| 23:27, 6 rêbendan 2007 | Metin Can (Nîqaş | Beşdarî) | 292 x 407 | 117 KB | Reverted to earlier revision
| 23:27, 6 rêbendan 2007 | Metin Can (Nîqaş | Beşdarî) | 292 x 407 | 117 KB | Reverted to earlier revision
| 22:10, 2 rêbendan 2007 | Metin Can (Nîqaş | Beşdarî) | 800 x 797 | 691 KB |
| 20:46, 26 berfanbar 2006 | Metin Can (Nîqaş | Beşdarî) | 292 x 407 | 117 KB |

- Edit this file using an external application

  See the setup instructions for more information.

## Lînkên vî wêneyî

Di van rûpelan de lînkek ji vî wêneyî re heye:

- Derwêş Serhedî
- Wêne:Derwês Serhedî.jpg

## Metadata

This file contains additional information, probably added from the digital camera or scanner used to create or digitize it. If the file has been modified from its original state, some details may not fully reflect the modified image.

Camera manufacturer | Canon
Camera model | Canon DIGITAL IXUS 430
Exposure time | 1/60 sec (0.0166666666667)
F Number | f/2.8
Date and time of data generation | 22:46, 24 kewçêr 2006
Lens focal length | 7.40625 mm
Orientation | Normal
Horizontal resolution | 75 dpi
Vertical resolution | 75 dpi
Software used | Adobe Photoshop CS Windows
File change date and time | 23:30, 8 rêbendan 2007
Y and C positioning | 1
Custom image processing | Normal process
Exposure mode | Auto exposure
White Balance | Auto white balance
Digital zoom ratio | 1
Scene capture type | Standard
Exif version | 2.2
Date and time of digitizing | 22:46, 24 kewçêr 2006
Image compression mode | 5
Shutter speed | 5.90625
Aperture | 2.96875
Exposure bias | 0
Maximum land aperture | 2.96875
Metering mode | Pattern
Flash | 89
Color space | sRGB
Focal plane X resolution | 8114.28571429
Focal plane Y resolution | 8114.28571429
Focal plane resolution unit | inches
Sensing method | One-chip color area sensor

Ji "http://ku.wikipedia.org../../../d/e/r/W%C3%AAne%7EDerw%C3%AAs_Serhed%C3%AE.jpg_c79e.html" hatiye standin.

Kategorî: CC-BY-SA-2.5

##### Views

- Wêne
- Guftûgo
- Revîzyona niha

##### Lêbigere