# Berkas:FordtaunusV4front.jpg

### Dari Wikipedia Indonesia, ensiklopedia bebas berbahasa Indonesia.

- Berkas
- Versi terdahulu
- Pranala

Tak tersedia resolusi yang lebih tinggi.

FordtaunusV4front.jpg‎ (420 × 320 piksel, ukuran berkas: 38 KB, tipe MIME: image/jpeg)

| Berkas ini berasal dari Wikimedia Commons. Berikut ini adalah deskripsi berkas dari halaman deskripsi di sana.

Front view of timing gears in a Ford Taunus V4 engine in a SAAB 96.

The (fibre) balance shaft gear (lower left) has lost its teeth due to bearing failure.
The other small (steel) gear is the crankshaft gear.
The largest (fibre) gear is the camshaft gear. It has twice the diameter of the crankshaft gear so it rotates at half the speed.

© photo, scan, upload MH 14:30, July 23, 2005 (UTC)

| This image has been released into the public domain by its author, Sonett72. This applies worldwide. In some countries this may not be legally possible; if so: Sonett72 grants anyone the right to use this work for any purpose, without any conditions, unless such conditions are required by law.

## Pranala

Halaman-halaman berikut memiliki pranala ke berkas ini:

- Camshaft

Diperoleh dari "http://id.wikipedia.org../../../f/o/r/Berkas%7EFordtaunusV4front.jpg_d81e.html"

##### Views

- Berkas
- Pembicaraan
- Revisi sekarang

##### Cari